- Qt Creator Documentation
- Debug C++ applications on VxWorks devices
- Qt Creator 18.0.0-beta1

Create kits for VxWorks devices ◦ Apply quick fixes

# Debug C++ applications on VxWorks devices

Note: Place all the library dependencies on the SD card. Debugging doesn't work from other locations, such as a mounted NFS directory.

Qt Creator only copies the application binaries and other deployable files to the root of the SD card. It doesn't preserve nor create the directory structure on the SD card.

To debug Qt applications, add the following line to your VxWorks source build (VSB) configuration:

     vxprj vsb config -s -add "_WRS_CONFIG_TCF_GDB_RSP=y"

To automatically start the GDB server on the device, add the following lines to your VxWorks image project (VIP) configuration:

     "INCLUDE_DEBUG_AGENT"
     "INCLUDE_DEBUG_AGENT_START"
     "INCLUDE_STANDALONE_SYM_TBL"

For more information, see Qt for VxWorks.

To set up debugging:

1. Activate a VxWorks kit for the project.
2. Go to Projects > Run.
3. In Run Settings, set Priority and Stack size.

4. In Environment, set the `LD_LIBRARY_PATH` variable to the location of the libraries on the SD card. If the path to the SD card is not `/sd0a`, set `VX_SDCARD_PATH` to the correct location.

To start debugging, press F5 or select Debug > Start Debugging > Start Debugging of Startup Project.

See also Activate kits for a project, Create kits for VxWorks devices, Debugging, and Qt for VxWorks.

Create kits for VxWorks devices ◦ Apply quick fixes